­­

Attendances by Others

Supplement to Installation specification ceda Standard Document C06

*#C25*

Commercial

**Using this document**

The highlighted areas indicate where you need to add your company details and then simply insert your logo in place of the ceda logo.

****

Introduction

This document is part of a suite of documents developed to provide members with standards that members are encouraged to adopt with the ultimate objective for them to become industry standards.

Scope

The purpose of this document is to provide a standard list of attendances required from other contractors on a construction site or as a basis for discussing specific requirements that may involve additional costs. Guidance notes to members are shown in italics.

Parking

On-site parking for engineers vehicles is to be provided free of charge. Where on-site parking is not available parking costs will be charged extra.

Welfare provision

On-site provision of toilet, washing and dining facilities is to be provided free of charge.

Health and Safety Induction

The contractor is to provide a health and safety induction talk (not exceeding one hour duration) to the installation team relevant to the site.

Off loading

Most equipment will be delivered on tail lift wagons and will be manually unloaded, however, in some instances, where the size of the equipment makes it impossible to unload in this way, it is expected that the contractor will provide heavy duty lifting/unloading facilities.

On site handling of equipment

Site movement of equipment will be on suitable pallet trucks or mobile dollies and therefore level access routes must be provided. Access is based on the kitchen being on the ground floor, however, where the kitchen is on a higher or lower floor it is expected that the client/contractor will provide suitable lifting facilities capable of transporting items up to 3 metres in length.

Protection of building finishes

Whilst every care will be taken in transporting equipment on site, it is the responsibility of others to protect building finishes on any access routes.

Working area

The areas where equipment is to be installed should be completely free from other trades and floor, wall and ceilings should be finished.

Suitable task lighting and electricity supply is to be provided.

Services

All services should be provided by other contractors to an agreed point within 1 metre of the final connection and terminated as requested by the equipment distributor.

Services should be tested and made live prior to the completion of installation so that commissioning can be carried out immediately following installation.

Water pipework should be thoroughly flushed out prior to installation commencing.

Grease management to comply with the Building Regulations 2010 paragraph 2.21 of section H1 to be provided by other contractors.

Kitchen equipment ventilation

Where the kitchen equipment ventilation is provided by others, the contractor shall commission this and provide to the distributor with a commissioning sheet including full details of the measured air volumes and flow rates for both extraction and make up air systems.